From 75e7d1301475d49311d14e202936c62df0c07d10 Mon Sep 17 00:00:00 2001
From: Klement Sekera <ksekera@cisco.com>
Date: Wed, 20 Sep 2017 08:26:30 +0200
Subject: IPv4/6 reassembly

Change-Id: Ic5dcadd13c88b8a5e7896dab82404509c081614a
Signed-off-by: Klement Sekera <ksekera@cisco.com>
---
 src/vnet/ip/protocols.def | 5 +++++
 1 file changed, 5 insertions(+)

(limited to 'src/vnet/ip/protocols.def')

diff --git a/src/vnet/ip/protocols.def b/src/vnet/ip/protocols.def
index 77fab31da05..4ec0bbc9284 100644
--- a/src/vnet/ip/protocols.def
+++ b/src/vnet/ip/protocols.def
@@ -158,5 +158,10 @@ ip_protocol (134, RSVP_E2E_IGNORE)
 ip_protocol (135, MOBILITY)
 ip_protocol (136, UDP_LITE)
 ip_protocol (137, MPLS_IN_IP)
+/*
+ * VPPs way of dealing with fragments is to mark them as 0xfe, to be picked
+ * by the corresponding nodes based on this protocol
+ */
+ip_protocol (0xfe, VPP_FRAGMENTATION)
 ip_protocol (255, RESERVED)
 
-- 
cgit 1.2.3-korg

