From 7cd468a3d7dee7d6c92f69a0bb7061ae208ec727 Mon Sep 17 00:00:00 2001
From: Damjan Marion <damarion@cisco.com>
Date: Mon, 19 Dec 2016 23:05:39 +0100
Subject: Reorganize source tree to use single autotools instance

Change-Id: I7b51f88292e057c6443b12224486f2d0c9f8ae23
Signed-off-by: Damjan Marion <damarion@cisco.com>
---
 src/vnet/ip/protocols.def | 162 ++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 162 insertions(+)
 create mode 100644 src/vnet/ip/protocols.def

(limited to 'src/vnet/ip/protocols.def')

diff --git a/src/vnet/ip/protocols.def b/src/vnet/ip/protocols.def
new file mode 100644
index 00000000000..77fab31da05
--- /dev/null
+++ b/src/vnet/ip/protocols.def
@@ -0,0 +1,162 @@
+/*
+ * Copyright (c) 2015 Cisco and/or its affiliates.
+ * Licensed under the Apache License, Version 2.0 (the "License");
+ * you may not use this file except in compliance with the License.
+ * You may obtain a copy of the License at:
+ *
+ *     http://www.apache.org/licenses/LICENSE-2.0
+ *
+ * Unless required by applicable law or agreed to in writing, software
+ * distributed under the License is distributed on an "AS IS" BASIS,
+ * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
+ * See the License for the specific language governing permissions and
+ * limitations under the License.
+ */
+/* Emacs editing mode -*-C-*-
+
+From http://www.iana.org/assignments/protocol-numbers
+
+PROTOCOL NUMBERS
+
+(last updated 18 October 2004)
+
+In the Internet Protocol version 4 (IPv4) [RFC791] there is a field,
+called "Protocol", to identify the next level protocol.  This is an 8
+bit field.  In Internet Protocol version 6 (IPv6) [RFC1883] this field
+is called the "Next Header" field.
+*/
+ip_protocol (0, IP6_HOP_BY_HOP_OPTIONS)
+ip_protocol (1, ICMP)
+ip_protocol (2, IGMP)
+ip_protocol (3, GGP)
+ip_protocol (4, IP_IN_IP)
+ip_protocol (5, ST)
+ip_protocol (6, TCP)
+ip_protocol (7, CBT)
+ip_protocol (8, EGP)
+ip_protocol (9, IGP)
+ip_protocol (10, BBN_RCC_MON)
+ip_protocol (11, NVP_II)
+ip_protocol (12, PUP)
+ip_protocol (13, ARGUS)
+ip_protocol (14, EMCON)
+ip_protocol (15, XNET)
+ip_protocol (16, CHAOS)
+ip_protocol (17, UDP)
+ip_protocol (18, MUX)
+ip_protocol (19, DCN_MEAS)
+ip_protocol (20, HMP)
+ip_protocol (21, PRM)
+ip_protocol (22, XNS_IDP)
+ip_protocol (23, TRUNK_1)
+ip_protocol (24, TRUNK_2)
+ip_protocol (25, LEAF_1)
+ip_protocol (26, LEAF_2)
+ip_protocol (27, RDP)
+ip_protocol (28, IRTP)
+ip_protocol (29, ISO_TP4)
+ip_protocol (30, NETBLT)
+ip_protocol (31, MFE_NSP)
+ip_protocol (32, MERIT_INP)
+ip_protocol (33, SEP)
+ip_protocol (34, 3PC)
+ip_protocol (35, IDPR)
+ip_protocol (36, XTP)
+ip_protocol (37, DDP)
+ip_protocol (38, IDPR_CMTP)
+ip_protocol (39, TP)
+ip_protocol (40, IL)
+ip_protocol (41, IPV6)
+ip_protocol (42, SDRP)
+ip_protocol (43, IPV6_ROUTE)
+ip_protocol (44, IPV6_FRAGMENTATION)
+ip_protocol (45, IDRP)
+ip_protocol (46, RSVP)
+ip_protocol (47, GRE)
+ip_protocol (48, MHRP)
+ip_protocol (49, BNA)
+ip_protocol (50, IPSEC_ESP)
+ip_protocol (51, IPSEC_AH)
+ip_protocol (52, I_NLSP)
+ip_protocol (53, SWIPE)
+ip_protocol (54, NARP)
+ip_protocol (55, MOBILE)
+ip_protocol (56, TLSP)
+ip_protocol (57, SKIP)
+ip_protocol (58, ICMP6)
+ip_protocol (59, IP6_NONXT)
+ip_protocol (60, IP6_DESTINATION_OPTIONS)
+ip_protocol (62, CFTP)
+ip_protocol (64, SAT_EXPAK)
+ip_protocol (65, KRYPTOLAN)
+ip_protocol (66, RVD)
+ip_protocol (67, IPPC)
+ip_protocol (69, SAT_MON)
+ip_protocol (70, VISA)
+ip_protocol (71, IPCV)
+ip_protocol (72, CPNX)
+ip_protocol (73, CPHB)
+ip_protocol (74, WSN)
+ip_protocol (75, PVP)
+ip_protocol (76, BR_SAT_MON)
+ip_protocol (77, SUN_ND)
+ip_protocol (78, WB_MON)
+ip_protocol (79, WB_EXPAK)
+ip_protocol (80, ISO_IP)
+ip_protocol (81, VMTP)
+ip_protocol (82, SECURE_VMTP)
+ip_protocol (83, VINES)
+ip_protocol (84, TTP)
+ip_protocol (85, NSFNET_IGP)
+ip_protocol (86, DGP)
+ip_protocol (87, TCF)
+ip_protocol (88, EIGRP)
+ip_protocol (89, OSPF)
+ip_protocol (90, SPRITE_RPC)
+ip_protocol (91, LARP)
+ip_protocol (92, MTP)
+ip_protocol (93, AX)
+ip_protocol (94, IPIP)
+ip_protocol (95, MICP)
+ip_protocol (96, SCC_SP)
+ip_protocol (97, ETHERIP)
+ip_protocol (98, ENCAP)
+ip_protocol (100, GMTP)
+ip_protocol (101, IFMP)
+ip_protocol (102, PNNI)
+ip_protocol (103, PIM)
+ip_protocol (104, ARIS)
+ip_protocol (105, SCPS)
+ip_protocol (106, QNX)
+ip_protocol (107, A)
+ip_protocol (108, IPCOMP)
+ip_protocol (109, SNP)
+ip_protocol (110, COMPAQ_PEER)
+ip_protocol (111, IPX_IN_IP)
+ip_protocol (112, VRRP)
+ip_protocol (113, PGM)
+ip_protocol (115, L2TP)
+ip_protocol (116, DDX)
+ip_protocol (117, IATP)
+ip_protocol (118, STP)
+ip_protocol (119, SRP)
+ip_protocol (120, UTI)
+ip_protocol (121, SMP)
+ip_protocol (122, SM)
+ip_protocol (123, PTP)
+ip_protocol (124, ISIS)
+ip_protocol (125, FIRE)
+ip_protocol (126, CRTP)
+ip_protocol (127, CRUDP)
+ip_protocol (128, SSCOPMCE)
+ip_protocol (129, IPLT)
+ip_protocol (130, SPS)
+ip_protocol (131, PIPE)
+ip_protocol (132, SCTP)
+ip_protocol (133, FC)
+ip_protocol (134, RSVP_E2E_IGNORE)
+ip_protocol (135, MOBILITY)
+ip_protocol (136, UDP_LITE)
+ip_protocol (137, MPLS_IN_IP)
+ip_protocol (255, RESERVED)
+
-- 
cgit 1.2.3-korg

